Article Navigation Back To Main Page Click Here for more articles |
Steps to Planting a Tree Correctly.
by: Hege Crowton
In planting trees, their mature height and spread must be considered before a selection is made. Tempting as are the nursery catalogues, it is necessary to choose carefully, especially on the average lot, because crowding spoils the growth and appearance of trees, particularly specimen trees. In general, it is wisest and most economical to plant young trees. Planting a mature tree is difficult and, if done professionally, costly. If, however, a mature tree is badly needed for a terrace or for screening, it may well justify the expense. What you are buying is the time it takes a smaller tree to mature. Today you can plant trees when in full leaf with the aid of new wilt-proof sprays that seal the leaves against moisture loss until the roots are established. This, however, costs money and entails greater risks than buying your tree and planting it in early spring (the best time) or late fall or winter. If you are planting a tree over 6 feet tall, it will suffer less setback if moved with a bur-lapped root ball. The soil preparation described in the previous chapter is helpful for most tree and shrub planting. But since the root system must have fertile soil when it is planted, special steps must be taken. Dig a hole 2 feet deep and at least 1 foot wider each way than the full spread of the roots. The bottom of the hole should be broken up with a pitchfork and thoroughly mixed with peat, leaf mould, loam, etc. Manure should be used sparingly and only on the top of the hole as it burns the roots. The deeper you can cultivate your hole, the better for your tree. Once it is planted, you can cultivate around it but not under the roots. If you strike a subsoil of building rubble or clay, which you are very apt to find anywhere near a house and in which a tree cannot grow, this subsoil must be removed and good soil, or better still, garden humus, substituted for it. If you are planting a seedling that is not balled and bur lapped, you will want to protect it by "heeling in" a vacant flower bed where it may be kept before planting as long as dormant. This means laying it on its side and covering the roots with good soil. When you take it from the soil, give it a mud bath or "puddle" it. Puddling protects the roots from exposure to air before planting and also from any air pockets which may exist after planting. Having filled the hole to the depth required by the roots of the plant, flood it with water to settle the soil at the bottom; when this has drained away, place the tree in the position in which it is to grow and settle the soil about it. Use a stick or shovel handle to work the soil around the roots, and make certain there are no air pockets. Spread the roots out naturally, planting the tree at about the same depth as in the nursery or its former location. When the hole is two-thirds full, trample it down and again fill with water. Don't firm down the remaining soil, so that the water will drain towards the trunk. A balled-and-bur lapped tree is one dug with a solid ball of rich, heavy loam in which it has been growing in the nursery for years, its root system thus amply covered and protected. The ball is firmed and held in place by a secure covering of twine and burlap. To plant it, set the tree in a hole that is a trifle lower than it stood in the nursery. Work the soil beneath this depth, as directed above. Dig the hole about twice the size of your ball and plant at once. If the ground is dry at planting time, fill the hole with water and let it soak away before planting. Cut the burlap at the top when you put the ball in place, rolling it back 3 or 4 inches. Plant ball, burlap and all—the burlap will soon rot away. If you are planting a big tree, it is transported in a truck, lowered to the ground by winches, rolled along a plank track on rollers and manoeuvred into the exact centre of the hole on a single board. A holding rope from the truck to the base of the tree trunk helps to position the tree. After the tree is planted, cutting back is proper. Cut back sharply at least one-third, pruning the branches. It is necessary to brace the tree with wire ropes so that the roots will not be broken by the wind. Use a single wire around the trunk and three guy wires. For the first year after planting, the more cultivation you can do the better. Keep weeds away, too, with straw or mulch, and straw manure mulch in the spring and fall will help keep the moisture in the ground. About the author: Hege Crowton is an expert copywriter. She is known for doing in-depth research before writing her articles. Many of her articles are posted on www.ezinecrow.com and she also does a lot of writing for www.CrowSites.com Copyright 2005 Gardeningcrow.com Circulated by Article Emporium

©2005 - All Rights Reserved