Article Navigation Back To Main Page Click Here for more articles |
Dealing with an Overheated Radiator
by: Terry Brown
Overheating is one of the most common breakdowns that autos encounter during the summer season. It happens when the temperature of the coolant exceeds the normal operating temperature range of the engine. Overheating has many causes. Idling under hot weather for prolonged periods can wreak havoc on the cars cooling system, because the water pump doesn't turn fast enough. Thus the coolant is not circulated, as it should be. Sometimes a leak may cause the coolant level to drop thus causing the radiator to overheat. Here are a few pointers for dealing with an overheated radiator: 1. Turn off the A/C. If the car is not seriously overheating, this will reduce the engine's temperature. The AC evaporator is located in front of the radiator, and it adds heat to the air going to your engine. The hotter the incoming air is, the less efficient the radiator will be. 2. Turn on your heater (set on highest temperature setting, with blower on highest setting). This will be uncomfortable for you, but it will cool the engine by transferring the heat to the air. Roll down the windows, and remember how 'hot' you'll get if your engine needs replacement! 3. If you're stuck in traffic, pull over and stop. Unless you're moving, very little cool air reaches the radiator. Open the hood and let the engine cool off. This takes time, so be patient. Use the time to go get a jug of water or antifreeze. 4. Check the overflow tank coolant level. If it's empty, the radiator is probably low on coolant. 5. Check the pressure of the system by wrapping a cloth around the upper radiator hose and squeezing it. If it's still under pressure (hot) it will not squeeze easily. Wait until it does. 6. Place a large cloth over the radiator cap, and carefully release the pressure. Serious burns can result from the hot coolant. If in doubt, wait until the engine cools completely. 7. If the coolant is low, start the engine, and slowly add the water or coolant necessary to fill it up. The engine must be running. Adding coolant to a warm engine can crack the block. By running the engine, the coolant keeps moving and reduces the chances of this type of damage occurring. Radiators are indispensable parts of any cooling system. They are designed to dissipate the heat, which the coolant has absorbed from the engine. However, like all auto parts, radiators are prone to damage and corrosion. As it is mostly made of metal and is in constant contact with liquids, radiators can break down over time due to corrosive forces. Defective radiators can spell doom for any engine. Irreparable damage can result if a malfunctioning radiator is not repaired or replaced immediately. If your radiator needs to be replaced, you can find aftermarket radiators that are more affordable but are nonetheless excellent in quality. Replacement radiators are available from the best auto parts suppliers online such as Auto Parts Inner. You can find top quality aftermarket Chevrolet Radiators for your Chevrolet automobile at very low prices. Not only that, they also have a wide array of Chevrolet Parts including Chevrolet A/C condensers, Chevrolet bumpers, Chevrolet catalytic converters, Chevrolet headlights, Chevrolet floor mats and other important Chevrolet parts. Auto Parts Inner’s array of top of the line Chevrolet parts are sourced from the most trusted auto parts makers in the country. All auto parts from Auto Parts Inner pass the stringent quality control standards that the company, a well-known resource of useful and relevant information, has set up. About the author: Terry Brown is a 32 year old from Houston Texas, and an enthusiast for anything auto related. He is currently employed as a market analyst by one of the top car parts company in the area. His automotive articles provide valuable source of information for auto enthusiasts like him as well as to those in need of automotive research. Circulated by Article Emporium

©2005 - All Rights Reserved